MODEL T-RP5 OIL-MINDER II CONTROL PANEL

Simplex elevator sump pump control panel

The Model "T-RP5" control panel provides reliable means of controlling one single phase or one three phase pump in elevator sump pits. The Stancor "T-RP5" control panel is designed to automatically pump fluid out of an elevator pit by means of a float switch and the oil sensing probe mounted on the pump. The control panel is equipped with electronic technology to sense emulsified oil and activate an alarm indicating that oil is being discharged from the pit.

PANEL COMPONENTS :

1. Enclosure Nema-4X with a gasketed screw down cover.

The control panel is equipped with marked terminal strips

for field wiring. (12"W x 14"H x 7" L)

2. The control panel is offered in 120, 208, 230 or 460 Volt

single or three phase. *Three phase and 460volt options require

a larger panel enclosure.

3. The control panel is equipped with a field adjustable oil

sensitivity switch with variable sensitivity settings, for indicating

oil present having a setting range of 1-10.

4. The control panel is equipped with a separate over-current relay

and field adjustable motor overload having a range of 5 to 15 amps.

(Factory set at the listed amps of the pump.)

5. RP (Remediation Provision) that consists of a dead man spring return Oil-Minder by pass switch mounted on the side of the control panel.

6. Float switch terminal block

7. Alarm and control circuit fuses

8. LED indicator lights for power on, oil detected and high water alarm.

9. Ground lugs

10. Circuit breakers

11. Individual dry contacts for remote monitoring of conditions of A, B, C, D & E.

A: The presence of oil in the sump pit when the pump is signaled to run.

B: High liquid level in the sump pit.

C: High amps or a locked rotor motor condition.

D: Loss of electrical power to the panel.

E: Pump run activation.

12. Alarm horn provides audio warning of alarm condition

13. Exterior Alarm reset and silence switch.

All control panels are inspected and tested before leaving the Stancor factory.

All control panels are constructed and tested to meet UL508 standards.

The Stancor T system meets ASME A17.1 ELEVATOR CODES

The Stancor T system meets The State Of Texas TDLR elevator requirments.

INDUSTRIAL SYSTEMS, INC.

1888 W. BITTERS RD.

SAN ANTONIO, TX 78248

P:210-493-4200